**1 D+H Mechatronic (english)**

**1.1 RT Series**

**1.1.1 SHEV operation panel - RT 45/R, red**

**Surface-mounted**

**Performance features:**

Operation panel for manually triggering a SHEV system in case of fire;

The operation panel is tested and certified in accordance with ISO 21927-9;

Shapely and extremely robust aluminium housing;

Can be used as main or auxiliary control panel;

Functions:

- SHEV OPEN, SHEV Reset

Display:

- Operational standby

- SHEV alarm triggered

- Fault indication

**Technical data:**

Supply: 24 V DC (18 - 28 V DC)

Type of protection: IP 40

Temperature range: -5 °C till +40 °C

Housing: Die-cast aluminium (surface-mounted housing)

Colour: Red (~ RAL 3000)

Dimensions (WxHxD): 129 x 138 x 39 mm

**Scope of supply:**

Lockable housing with operation unit, break-type glass, key, designation labels in 32 languages

Brand: D+H Mechatronic AG

Type: RT 45/R

[Planning Support](https://www.dh-partner.com/int/en/service/planning-support)

|  |  |
| --- | --- |
| **Artikelnr.:** | 65.403.25 |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | | **Quantity:** |  | | Stk | |  |  | | --- | --- | | **Preis:** |  | | € | |  |  | | --- | --- | | **TP:** |  | | € |